WCI Stack Certification Test Registration Form

|  |
| --- |
| Manufacturer - Corporate Information |
| Company |  |
| Street Address |  |
| City |  |
| State, Province |  |
| Postal code |  |
| Country |  |

|  |
| --- |
| Manufacturer - Requesting Division and Site Information |
| Division Name |  |
| Street Address |  |
| City |  |
| State, Province |  |
| Postal code |  |
| Country |  |

|  |
| --- |
| Testing Contact Regarding Testing and Registration |
| Name |  |
| Phone |  |
| Fax |  |
| Email |  |
| Time zone |  |

|  |
| --- |
| Purchasing Contact Regarding Billing and Payment |
| Bill To Name |  |
| Bill To Phone |  |
| Bill To Fax |  |
| Bill To Email |  |
| Bill To Time zone |  |
| Purchase Order # |  |

|  |
| --- |
| Product Description |
| Selling Product name |  |
| Selling Product code |  |
| Selling Product description(for the WCI web site) |  |
| Product http reference(optional, for the web site) |  |
| Internal Product Code (if prototype) |  |
| Stack firmware version(Software\_Revision\_Information) |  |
| Radio Transceiver (Manufacturer, Model Number) |  |
| Stack Microprocessor(Manufacturer, Model Number, Memory Configuration) |  |
| Stack test hardware(Model name if applicable, or other description |  |
| Stack Binary/Stack Binary Hash |  |

|  |
| --- |
| Stack Test Requirements not covered by STK 2010 |
| [DL-PHY.1] | The PHY shall support channels 11-25, at a power level as indicated in DeviceCapability.RadioTransmitPower. |
| [DL-PHY.4] | Actual transmit power shall not exceed RadioTransmitPower by more than 4 dB. |
| [DL-PHY.5] | RadioTransmitPower shall be validated at 0 dBm, dlmo11a.RadioTransmitPower, and a value halfway between.  |
| [DL-TS.5] | The DL shall not wake up too late (WakeupDPDU and WakeupAck) or time out too early (TimeoutDPDU and TimeoutAck) |

Vendor will provide test results as evidence of compliance to these requirements.

|  |
| --- |
| Product Configurations (if applicable) |
| Product name |  |
| Product code |  |
| Product description(for the WCI web site) |  |
| Product http reference(optional, for the web site) |  |

Note: Please use this table one or multiple times if exactly the same Stack is to be listed on the WCI web site under multiple configurations (names and/or product codes). An identical Stack with a different configuration and firmware is considered a family member.

|  |
| --- |
| Stack Binary/ Stack Binary Hash |
| Hash: |  |

Please perform a hash of the stack binary using the Microsoft File Checksum Integrity Verifier (FCIV). This is a free tool available here: <http://www.microsoft.com/en-us/download/details.aspx?id=11533>

|  |
| --- |
| Checklist of Items required for testing to commence |
| Must be Included with Request form | --------------------------------------------------------------- |
| SS.ini file along with text description |  |
| Signed agreement with WCI Test Lab |  |
| PO Number for payment |  |
| Completed Request form (this form) |  |
| Stack setup instructions (including detailed instructions to configure iBoot) |  |
| Duplicate (2) hardware test configurations. 1 to be retained by WCI. |  |
| All hardware and software necessary to update firmware at WCI HQ |  |
| Complete set of logs |  |
|  |  |

|  |
| --- |
| Stack Test Service and Fee Schedule in US Dollars(circle one) |
|  | Fees |
| Stack Test Type | Test Service | Logo & Registration |
| 1 | First time stack test or re-run of first time test for single stack certification | 9,000 | 9,000 |
| 2 | Supplier self-test review and administration | 3,000 | 3,000 |
| 3 | Hourly rate for WCI test agency engineering/test support services | 225 |
|  |